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Henan Zhaobang Cold Chain Equipment Co., Ltd.
Thank you for purchasing our product.

To ensure proper operation and optimal performance,

please read this manual carefully before use.
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summary
1. This product employs a fully enclosed compressor. It utilizes the environmentally friendly refrigerant R290 and is properly matched with an air-cooled refrigeration system, ensuring uniform internal temperature distribution within the unit.
2. The glass is made of ultra-clear tempered glass, offering an elegant and aesthetically pleasing appearance with perfect transparency that allows food items stored inside to be clearly visible at a glance.
3. This device is intended for household and similar uses, such as:
—The kitchen area in a store, office, or other workplace;
—Customers of farms, hotels, motels, and residential environments;
—A family inn-style environment;
—Food service industry and similar non-retail applications.
Structure and Parts (Examples)          
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pay attention to
1. The electrical schematic diagrams and parameters shall follow those specified on the product nameplate.
2. The product may be improved without prior notice.
3. If the power cord is damaged, it must be replaced by the manufacturer, its authorized representative, or qualified personnel. Only professional after-sales service personnel are permitted to repair the damaged cord using specialized tools.
4. This device shall not be used by individuals with physical, sensory, or mental disabilities, or lacking sufficient experience and knowledge for its operation (including children), unless supervised or guided by a person responsible for their safety regarding the device's usage.
5. Children must be supervised to ensure they do not play with this device.
6. This user manual is not applicable to individuals with physical disabilities, sensory or mental disorders (including children), or those lacking experience or knowledge.
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-The electrical schematic diagram and parameters shall be subject to those on the product nameplate. 
-The product may be improved without notice. 
-Except for the methods recommended by the manufacturer, no mechanical equipment or other means shall be used to accelerate the defrosting process.
-Do not damage the refrigeration circuit.
-Electrical appliances shall not be used in the food storage compartment of the appliance, except for the types recommended by the manufacturer.
-Warning: Do not store explosives, such as combustion accelerators, inside the device.
-When placing the equipment, make sure the power cord is not stuck or damaged.
-No portable multi-socket or portable power source shall be placed on the back of the appliance.
-The refrigeration system is under high-pressure conditions and must not be altered. Contact qualified service personnel before any modifications.
-Warning: Our products contain flammable cyclopentane as a foaming agent. Discarded equipment must be returned to the manufacturer or a certified recycling facility.
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Do not dispose of electrical appliances without proper classification; consult the local government to confirm whether a recycling system is available.If electrical appliances are disposed of as waste, hazardous substances can leach into groundwater and enter the food chain, thereby harming your health.When new electrical appliances replace old ones, the seller is obligated to recall the old appliances free of charge for disposal.
Transport and Placement
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Usage and Precautions
Before Use
The device operates on a 220–240 V independent power socket and features dedicated grounding.After the device is activated, check manually whether cold air is blowing from the outlet. If cold air is present, the food can be placed inside the device.

Precautions

Shortening the door opening time or reducing the frequency of door openings helps maintain the chamber temperature.

Do not block the air outlet and inlet to maintain proper air circulation inside the unit.

Food should not be stored in overly crowded areas to avoid compromising cooling efficiency.

Adjust the height of the grid frame appropriately to suit food storage;

Hot food must be cooled to room temperature before being placed in the refrigerator.

During a power outage, minimize door openings to maintain the internal temperature of the box.

Do not touch the compressor to avoid burns.
Principle of the Refrigeration System and Electrical Circuit Diagram
The refrigeration principle of a compressor system consists of compression, cooling, throttling, and vaporization.
The refrigerant is compressed by the compressor in the condenser, then throttled through the capillary tube, and finally vaporizes in the evaporator.
When the refrigerant circulates within a closed refrigeration system, the compressor draws in the refrigerant that has passed through the evaporator and absorbed its heat. Under the action of the compressor, the refrigerant is converted into a high-pressure, high-temperature gas. In the condenser, the refrigerant releases its heat to the air while beginning to liquefy again; it then enters the low-pressure evaporator via a capillary throttling valve. As the liquefied refrigerant suddenly loses pressure and evaporates rapidly, it absorbs a significant amount of heat from the refrigeration unit's interior. The compressor subsequently draws in the low-pressure, low-temperature vaporized refrigerant, and this cycle repeats to achieve the cooling objective.

maintenance and repair
pay attention to 
Regular maintenance and keeping the freezer clean are essential.

Unplug the power supply before maintenance.

Do not use damaged plugs or sockets that are too loose to prevent electric shock and short circuits.

Do not shake the freezer or use alkaline cleaners, soap, gasoline, acetone, or brushes.
Clean the exterior
Clean the exterior of the refrigerator with a soft cloth dipped in a neutral dishwashing detergent, then dry it

with a soft, dry cloth.
3. Clean the interior
Remove the frame and clean it with water.
4. Long-term disuse of the cold storage unit
Remove all food items from the device and disconnect the power supply.

Thoroughly clean both the interior and exterior of the freezer, then open the door until it is completely dry.
The glass is prone to breaking and should be kept out of reach of children.
Question Answer (Branch, with corresponding causes and methods)
	question
	Possible causes of the malfunction
	Simple Treatment Method

	No cooling
	Is it plugged into power?
	Check the contact between the plug and the socket.

	
	Is the fuse broken? Is there a power outage?
	Check the power status of the viewing environment.

	The cooling performance is unsatisfactory.
	Is it exposed to sunlight? Are there any heat sources nearby?
	Move to a corner where sunlight does not shine directly and there are no heat sources nearby.

	
	Is the surrounding ventilation poor?
	Leave at least 10 cm of space around the product for heat dissipation and ventilation.

	
	Is the door properly closed? Has it been left open for an extended period?
	Check that the cold cabinet door is closed.

	
	Is the seal deformed or damaged?
	Check the seal condition of the cold cabinet door.

	
	Adjust the electronic digital temperature control?
	If the electronic temperature control settings have been adjusted, restore them to factory defaults.

	The noise is loud.
	Is the cold cabinet not placed level?
	Check and adjust the placement level of the cold cabinet.

	
	Has the cold cabinet hit a wall or something else?
	There should be no objects directly adjacent to the cold cabinet; a space of at least 10 centimeters must be maintained.

	
	Are any parts of the cold cabinet loose?
	Inspect the interior of the cold cabinet; visible looseness or detachment of components such as the grid structure can be directly observed.

	If simple troubleshooting doesn't resolve the issue, please contact your local service center for assistance.


pay attention to ：
The following phenomenon does not indicate a problem: hearing a gurgling sound of water while the freezer is operating is a normal occurrence as the refrigerant circulates within the system.
During humid seasons, condensation may form on the exterior of refrigerators due to high air humidity; simply wipe it dry with a cloth.
For detailed circuit diagrams and parameters, refer to the cabinet nameplate.
Description of the content and state of harmful

substances in the product
Appendix: Statistical Table of Toxic and Harmful Substances in Refrigerated Display Cases
	Part Name
	hazardous material

	
	Lead (Pb)
	mercury （Hg）
	cadmium （Cd）
	hexavalent chromium
(Cr(VI))
	Polybrominated biphenyl
(PBB)
	Polybrominated diphenyl ethers
(PBDE)

	Box assembly component
	O
	O
	O
	O
	O
	O

	Door body assembly
	O
	O
	O
	O
	O
	O

	heat insulating material
	O
	O
	O
	O
	O
	O

	Internal components of the box
	O
	O
	O
	O
	O
	O

	Final assembly component
	O
	O
	O
	O
	O
	O

	Compressor
	X
	O
	O
	O
	O
	O

	Pipeline components
	
	O
	O
	O
	O
	O

	Wiring Type
	O
	O
	O
	O
	O
	O

	Electronics components
	X
	O
	O
	O
	O
	O

	Packaging and Printing
	O
	O
	O
	O
	O
	O

	O: Indicates that the concentration of this hazardous substance in all homogeneous materials of the component complies with the limits specified in the current effective version of GB/T 26572.
Please provide the following.
X: Indicates that the concentration of the hazardous substance in at least one homogeneous material of the component exceeds the limits specified in the current effective version of GB/T 26572.
Limitation requirements.

	        The "environmentally friendly service life" of this product is 15 years, a duration determined by the company based on the product's design specifications.
        The "environmentally friendly service life" is only valid when the product is used under the normal conditions specified in its instruction manual.


The components listed in the detail table summarize the main components included in different product models. Whether this product includes a given component depends on the specific product.
The actual configuration of the product shall prevail.
For items not listed in the detailed table, other components and their homogeneous materials contained in this product do not contain any harmful substances.
All components containing hazardous substances in the detailed list, along with their homogeneous materials, comply with the stringent restrictions on hazardous substance usage under the EU RoHS regulation.
Please use it with confidence.
Friendly reminder: To protect the environment, as a consumer, you are responsible for disposing of this product or its components properly after they reach the end of their service life.
Separate household waste and deliver it to qualified recycling stations, where the waste will be sorted, dismantled, and recycled in accordance with national regulations.
Reutilization and other treatments.
This product has obtained conformity assessment in accordance with the requirements specified in the announcement jointly issued by the State Administration for Market Regulation and the Ministry of Industry and Information Technology regarding the "Implementation Arrangement for the Conformity Assessment System on the Restriction of Hazardous Substances in Electrical and Electronic Products." The conformity assessment certification is indicated by the RoHS label adjacent to the product nameplate.
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Place in a dry location The cold cabinet should be placed in a dry location.





Handle with care First, unplug theconnector. During transportation, ensure the cabinet is not tilted more than 45 degrees.





Good ventilation Place the refrigerator in a well-ventilated area. For the first use or after transportation, wait for 2 hours before powering it on.





sufficient room The distance between both sides and the back of the cold cabinet and the wall or other objects shall be no less than 10 cm. An excessively small surrounding air circulation space will increase the load on the cold cabinet.





Keep away from heat sources Do not expose the refrigerator directly to sunlight. To prevent a decline in cooling performance, avoid placing it near any heat source.








Do not apply excessive pressure


Do not place heavy objects on the top surface of the refrigerator.





Place steadily Remove the packaging and place the freezer in a flat, sturdy location.





Do not drill Do not drill holes in the refrigerator or install any other items on it.





Preparation and Power Supply For normal use: AC 220-240V,50Hz, single-phase power supply





Independent power outlet


Do not share a socket between the cold cabinet and other electrical appliances, as this may cause power overheating and pose a fire hazard.





Protect the power cord Do not damage the power cord, as this may cause electrical leakage and fire.





Do not rinse with water Do not rinse the surface of the cold cabinet, as this may cause electrical leakage.





Keep away from flammable and explosive materials 


Do not place any flammable or explosive materials,


 such as ether, alcohol, gasoline, adhesive, or 


explosives, inside the cold cabinet. Keep hazardous 


substances away from the cold cabinet.





Spraying flammable materials Do not spray flammable materials near the freezer, as this may cause a fire.





Chemical substancesChemical substances must not be stored in refrigerators.





power cut After a power outage or unplugging the plug, wait for 5 minutes before powering on the cold cabinet again.
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